	Specification
	10g
	20g
	30g

	Model
	QRR0.01G/S
	QRR0.02G/S
	QRR0.03G/S

	Agent dosage
	10 g
	20 g
	30 g

	Protected volume*
	Up to 0.1 m³
	Up to 0.2 m³
	Up to 0.3 m³

	Aerosol generation duration
	≤6 s
	≤6 s
	≤6 s

	Service life
	10 years
	10 years
	10 years




	Specification
	Details

	Activation method
	Thermal activation; no external power required

	Activation temperature
	170°C

	Activation response
	Aerosol generation starts within 15 seconds after reaching the activation temperature

	Mounting options
	35 mm DIN-rail mounting or customized 3M adhesive side mounting

	Housing color
	Red

	Thermal probes
	Two probes, located at the top and bottom

	Probe cable length
	Standard: 10 cm per probe; customizable from 10 to 50 cm

	Operating temperature
	−50°C to +90°C

	Humidity tolerance
	<95% RH, non-condensing



